PRODUCT CARD DOUBLE SWING
Cat. no. 601

Swing dimensions:
Length: 3.8 m
Width: 2.3 m
Height: 2.2 m
Minimum space: 3.1 x 7.3 m
Age group: 0 to 14 years
Free fall height: 1.3 m

Guidelines for materials and technology of construction of the device.

The struts and the top beam, which form the swing structure, are made of 76.1 mm diameter stainless steel tube. The stainless steel is grade 0H18N9. The foundations are made as concrete footings founded at a depth of 0.6 m. The seats are made of a steel insert covered with EPDM rubber. It is possible to fit a child-safe seat. Fasteners, chains and slings are made of stainless steel. A maintenance-free roller bearing is used in the slings. End caps are made of plastic.

The fall area of the device should be made on a surface in accordance with EN 1176-1:2017.